Q3 driver package for CUSTOM ENGINEERING Q3 printer:

Windows 2000.
Windows XP.
Windows 2K3.
Windows Vista 32bit.
Windows Vista 64bit.
Windows 7 32bit.
Windows 7 64bit.

Installation procedure:
a) Serial interface
For a serial interface printer (W2k, XP, 2K3, Vista and 7) you can execute the standard
printer installation procedure or follow the automatic wizard procedure.
For standard printer installation the needed file are stored into: "..\TempDrv" directory.
b) USB interface
Follow the automatic wizard procedure.

This driver supports printer:
"CUSTOM Q3"

The "CUSTOM Q3" prints on a paper width size of 80mm but the printable
region width is 76mm.

This printer supports some page format:

"Q3 Roll"
"Q3 Roll Short"
"Q3 80mm"
"Q3 120mm"
"Q3 160mm"
"Q3 200mm"
"Q3 240mm"
"Q3 280mm"
"Q3 400mm"

If the system driver properties section shows these page formats and other not here
specified, you must select only the above mentioned pages format.

Note about BlackMark Feature:
 we suggest to use "Q3 Roll" page format when You are using Notch Alignmemnt.

